DRC Rules Export File for PCB: P:\QUA_2475\Tester\HW\PCB\stimuliBoard.PcbDoc
RuleKind=Width|RuleName=C71|Scope=Board|Minimum=7.87
RuleKind=Width|RuleName=GND|Scope=Board|Minimum=7.87
RuleKind=Width|RuleName=C72|Scope=Board|Minimum=7.87
RuleKind=Width|RuleName=D50|Scope=Board|Minimum=7.87
RuleKind=Width|RuleName=VIO|Scope=Board|Minimum=7.87
RuleKind=Width|RuleName=V24|Scope=Board|Minimum=7.87
RuleKind=Width|RuleName=VIN|Scope=Board|Minimum=31.50
RuleKind=Width|RuleName=VCC_ETH|Scope=Board|Minimum=7.87
RuleKind=ShortCircuit|RuleName=ShortCircuit|Scope=Board|Allowed=0
RuleKind=SolderMaskExpansion|RuleName=SolderMaskExpansion|Scope=Board|Minimum=4.00
RuleKind=Width|RuleName=VCC|Scope=Board|Minimum=7.87
RuleKind=Clearance|RuleName=Clearance|Scope=Board|Minimum=7.87
RuleKind=Width|RuleName=Signal|Scope=Board|Minimum=7.87
RuleKind=Width|RuleName=VCC_ANA|Scope=Board|Minimum=7.87
RuleKind=Width|RuleName=VCC_SD|Scope=Board|Minimum=7.87
RuleKind=Width|RuleName=VIN_DIGI|Scope=Board|Minimum=7.87
RuleKind=Width|RuleName=F2_1|Scope=Board|Minimum=7.87
